**Determining the Correct Pressure**

**With Your Gun and Your Paint**

Don’t adjust the paint, Adjust the spray gun.

**•** Hold the gun about **6-8** inches from a piece of masking paper.

**•** Set the pressure at **30** psi, pull the trigger back fully and release.

**•** Repeat at **5** psi increments until two identical patterns are produced.

No single spray gun or setup will work for the entire project.

Don’t adjust the paint so that the equipment works properly.

The equipment should work as you need it to.

If the result is not satisfactory, change equipment and/or equipment settings to improve results.

When in doubt about spray equipment, ask Shawnee Paint.