**Caution:** Wear the proper safety protection when sanding, cleaning, mixing and spraying all materials included within this process.

PD-0420

SPRAY GUN CLEANUP

**QUICK CHANGE CUP SYSTEM**

1. Use

 a disposable spray gun cup or a cup with a disposable liner.

1. Invert

 spray gun, pull trigger to release paint and remove gun cup. Dispose of leftover paint.

1. Remove

air cap and clean it with a soft bristle brush and cleaning solvent.

1. Trigger

the spray gun and remove the fluid tip with fluid tip wrench and clean it with a soft bristle brush and cleaning solvent.

1. Remove

the fluid needle and wipe it clean with cleaning solvent.

1. Flush

spray gun with cleaning solvent through the hole where the gun cup attaches. Flush until clean.

1. Wipe

all parts and spray gun body dry with soft cloth.

1. Reinstall

fluid needle while triggering the gun.

1. Lubricate

according to spray gun manufacturer with approved spray gun lube.